JOBSITE SAFETY INSPECTION

Inspector:______________________________________________Date:_________________

Location:____________________________________________________________________

										Yes		No

1.	First-Aid Kit: Should be conspicuously located and 
	contain adequate supplies.						____		____
	Comments:_____________________________________________________________
2.	First-Aid Personnel: Should be present on jobsite if not 
	in close proximity to a doctor or hospital. 				____		____
	Comments:_____________________________________________________________
3.	Emergency Phone Numbers: Should be posted in 
	conspicuous locations near phone. 					____		____
	Comments:_____________________________________________________________
4.	OSHA Poster: Should be conspicuously located where 
	employees can see. 							____		____
	Comments:_____________________________________________________________
5.	OSHA 200/300 Injury/Illness Log: Should be on file or 
	posted in jobsite trailer.						____		____
	Comments:_____________________________________________________________
6.	Jobsite Trailer: Should be maintained in a reasonably 
	neat condition. 							____		____
	Comments:_____________________________________________________________
7.	Trash Containers:  Should be provided and used, 
	emptied as necessary. 						____		____
	Comments:_____________________________________________________________
8.	Tool Storage Facilities: Should be kept reasonably
	neat and free of tripping hazards.					____		____
	Comments:_____________________________________________________________
9.	Project Materials: Should be stored in a safe manner 
	and safely accessible. 						____		____
	Comments:_____________________________________________________________
10.	Scrap Materials, Trash and Debris: Should be in 
	designated areas and hauled off when necessary. 			____		____
	Comments:_____________________________________________________________
11.	Fire Extinguisher(s): Should be charged and readily 
	available in case of an emergency.					____		____
	Comments:_____________________________________________________________
12.	Hard Hats: Should be worn by all persons while 
	on the jobsite.								____		____
	Comments:_____________________________________________________________
13. 	Shirts, Shoes, Boots: Should be worn by all persons on jobsite.
	NO OPEN-TOED OR CANVAS SHOES.				____		____
	Comments:_____________________________________________________________

										Yes		No

14.	Personal Protective Equipment: Such as gloves, rubber boots, 
	etc., should be worn as dictated by the work being performed.  	____		____
	Comments:_____________________________________________________________
15.	Eye Protection: Should be available and used 
	when needed for protection. 						____		____
	Comments:_____________________________________________________________
16.	Respirators: Should be available and used as required.		____		____
	Comments:_____________________________________________________________
17.	Ear Protection: Should be available and used when required.	____		____
	Comments:_____________________________________________________________
18.	Compressed Gas Cylinders: Should be in upright, secured 
	position when not in use, separated from heat, and capped.  	____		____
	Comments:_____________________________________________________________
19.	Ladders: Should be in good condition, tied off, and extending 
	3 feet above landing when in use. 					____		____
	Comments:_____________________________________________________________
20.	Electrical Cords & Tools: All 15 - 20 amp electrical cords, 
	and tools should be tested and properly taped as described 
	in the company’s Assured Equipment Grounding Program.
	Exceptions: Does not apply if using GFCI’s or double-insulated 
	tools. 									____		____
	Comments:_____________________________________________________________
21.	Flammable Liquids: Should be stored in approved 
	containers, contents identified, stored in approved 
	flammable storage cabinets, and warning signs posted.  		____		____
	Comments:_____________________________________________________________
22.	Trenches and Excavations: 5 or more feet deep should be 
	shored or back sloped and adequately barricaded.			____		____
	Comments:_____________________________________________________________
23.	Machine Guards: Should be on saws, grinders, 
	exposed belts, etc. 							____		____
	Comments:_____________________________________________________________
24.	Caution Lights: Should be installed on all company trucks 
	and around open trenches when necessary.  				____		____
	Comments:_____________________________________________________________
25.	Utility Work Traffic Signs: Should be in good condition 
	and displayed properly. 					____		____
	Comments:_____________________________________________________________
26.	Material Safety Data Sheets (MSDS): Should be kept with 
	supervisors and displayed in the jobsite trailers or field offices.	____		____
	Comments:____________________________________________________________
27.	Subcontractors: Should be in compliance with all safety item.  
	If they are not in compliance, they should be notified immediately. ____		____
	Comments:_____________________________________________________________